,TS Frame##Other##,Ampere Ratings##Other##,Basic Transfer Type##Other##,Poles##Other##,Neutral Type##Other##,UL Enclosure Type Rating##Other##,Mounting Type##Other##,H##Length##Inches,W##Length##Inches,D##Length##Inches,Ventilation Location##Other##,Conductor Entry##Other##,Power Terminal Conductor Range Phase and N (Al/Cu)##Other##,Power Terminal Locations##Other##,Ground Terminal Conductor Range (Al/Cu)##Other##,Ground Bus 20 Percent Rated##Other##,Model Number##Other##
2600A-Open Transition Transfer Switch-2P,G,2600,TS,2,"None,Solid,Switched,Overlapping",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TS-2600-2P
2600A-Open Transition Transfer Switch-3P,G,2600,TS,3,"None,Solid,Switched,Overlapping",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TS-2600-3P
3000A-Open Transition Transfer Switch-2P,G,3000,TS,2,"None,Solid,Switched,Overlapping",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TS-3000-2P
3000A-Open Transition Transfer Switch-3P,G,3000,TS,3,"None,Solid,Switched,Overlapping",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TS-3000-3P
2600A-Delayed Transition Transfer Switch-2P,G,2600,DTS,2,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTS-2600-2P
2600A-Delayed Transition Transfer Switch-3P,G,2600,DTS,3,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTS-2600-3P
3000A-Delayed Transition Transfer Switch-2P,G,3000,DTS,2,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTS-3000-2P
3000A-Delayed Transition Transfer Switch-3P,G,3000,DTS,3,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTS-3000-3P
2600A-Closed Transition Transfer Switch-2P,G,2600,CTS,2,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTS-2600-2P
2600A-Closed Transition Transfer Switch-3P,G,2600,CTS,3,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTS-2600-3P
3000A-Closed Transition Transfer Switch-2P,G,3000,CTS,2,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTS-3000-2P
3000A-Closed Transition Transfer Switch-3P,G,3000,CTS,3,"None,Solid,Switched",3R,Free Standing,95.4,40,69.8,Front / Rear,Bottom,(12) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTS-3000-3P
