SoMachine V4.3
Vijeo Designer V6.2 SP6.1 Update

Release Notes
.

Software Version:	6.2.6.1008	
Development Stage:	Final	
Build:	18.05.03.01	
Release Date:	03. May 2018	

This document contains important information about the SoMachine software. 
Read the complete document before you run the product.

The information provided in this documentation contains general descriptions and/or technical characteristics of the performance of the products contained herein. This documentation is not intended as a substitute for and is not to be used for determining suitability or reliability of these products for specific user applications. It is the duty of any such user or integrator to perform the appropriate and complete risk analysis, evaluation and testing of the products with respect to the relevant specific application or use thereof. Neither Schneider Electric nor any of its affiliates or subsidiaries shall be responsible or liable for misuse of the information contained herein. If you have any suggestions for improvements or amendments or have found errors in this publication, please notify us. 
You agree not to reproduce, other than for your own personal, noncommercial use, all or part of this document on any medium whatsoever without permission of Schneider Electric, given in writing. You also agree not to establish any hypertext links to this document or its content. Schneider Electric does not grant any right or license for the personal and noncommercial use of the document or its content, except for a non-exclusive license to consult it on an "as is" basis, at your own risk. All other rights are reserved. 
All pertinent state, regional, and local safety regulations must be observed when installing and using this product. For reasons of safety and to help ensure compliance with documented system data, only the manufacturer should perform repairs to components.
When devices are used for applications with technical safety requirements, the relevant instructions must be followed. 
Failure to use Schneider Electric software or approved software with our hardware products may result in injury, harm, or improper operating results. 
Failure to observe this information can result in injury or equipment damage.

© 2017 Schneider Electric. All Rights Reserved.

Table of contents
1.	System Requirements
1.1.1.	PC Software Requirement
2.	IMPORTANT INFORMATION
2.1.1.	Installation
2.1.2.	Improvements inside Vijeo Designer 6.2 SP6.1
2.1.3.	Limitations
2.1.4.	List of integrated components

1.	System Requirements
1.1.1.	PC Software Requirement 
This addon is dedicated to, and must be installed in conjunction with, SoMachine V4.3 only.

	
2.	IMPORTANT INFORMATION
2.1.1.	Installation
The addon is delivered as a container file in SECO format and can  be installed on top of SoMachine V4.3. 

Use the SoMachine Configuration Manager (SCM) to install this addon.

In Windows Explorer, double-click the SECO file delivered through this Patch, which will start SCM and the installation.

Alternatively, you can start SCM manually, change to the tab "Add-Ons/Patches" and choose "From File >" to open the delivered SECO file.

The installation of this addon requires administrator privileges to start.

Note:
Former versions of Vijeo Designer  will be uninstalled at first. Afterwards Vijeo Designer SP6.1 will be installed.
2.1.2.	Improvements inside Vijeo Designer 6.2 SP6.1
New features
•	Support new Magelis displays (and XL display) HMIDT752 and HMIDT952 on HMIG5U2 in SoMachine
•	Support new Magelis iPC
o	HMIPSP
o	HMIPEP
o	HMIPSO
o	HMIBMU
o	HMIBMP
•	Improved Microsoft Windows10 Pro 32bit/64bit support
•	Support resolution on Magelis iPC HMIBMU and HMIBMP:
o	800 x 600 (SVGA)
o	1280 x 720 (HD720)
o	1280 x 800 (WXGA)
o	1280 x 1024 (SXGA)
o	1440 x 900 (WSXGA)
o	1600 x 1200 (UXGA)
o	1680 x 1050 (WSXGA+)
o	1920 x 1200 (WUXGA)
o	2560 x 1600 (WQXGA)

Quality improvements
•	Improve robustness of HMSCU by preventing USB event file corruption due to the power interruption (which could be provoked by backing-up Event Log groups).
•	Improve robustness of HMSCU by preventing SRAM alarm file corruption due to power interruption (which could be provoked by backing-up Alarms)
•	Improve robustness of HMISCU (runtime) when using function block READ_VAR (of library PLCCommunication) for Modbus communication (thus avoiding loss of read registers).
•	Improve robustness of Vijeo-Designer by accepting also variables with specific or empty namespace attribute to be shared via SoMachine’s symbol configuration.
•	Improve robustness on HMIS5T: the connection via Ethernet to a controller will be reestablished after a temporary disconnection.
•	Allow to convert a  HMI “with Control” into one without control within the Standalone version of Vijeo Designer. 
This implies performing first an export from SoMachine into a Vijeo Designer vdz file, followed by the conversion within the “Standalone” version of Vijeo Designer, followed by the import of the new vdz file into SoMachine.
•	Avoid the dialog “Security has been set up on the target machine” (prompting for an user and password) when downloading an application via Vijeo Designer (“Download Target”), in case security was not set-up.
2.1.3.	
Limitations
•	“Performing an ‘Online Change’ command on a HMI SCU controller may lead to the situation, that the controller application will not reboot (no boot application on controller).
Therefore after performing one or several ‘Online Change’ commands you have to perform a Full Download for rebooting successfully.”

2.1.4.	List of integrated components
Component	Version	
OptimizedRepository	4.3.0.2 (18.2.2.1)	
Vijeo	6.2.6.1008 (18.3.20.3)