$ EZ-EDS Version 3.23.1.20171205 Generated Electronic Data Sheet

[File]
        DescText = "Power Logic PM55XX Series meter";
        CreateDate = 12-06-2017;
        CreateTime = 09:22:46;
        ModDate = 01-29-2018;
        ModTime = 08:44:27;
        Revision = 1.1;
        HomeURL = "http://www.schneider-electric.com";

[Device]
        VendCode = 243;
        VendName = "Schneider Electric";
        ProdType = 43;
        ProdTypeStr = "Generic Device";
        ProdCode = 10241;
        MajRev = 1;
        MinRev = 1;
        ProdName = "PM55XX";
        Catalog = "PowerLogic PM55XX Meter";
        Icon = "PM55xx.ico";
        IconContents =
                "Qk1WIQAAAAAAADYAAAAoAAAANQAAADUAAAABABgAAAAAACAhAAB0EgAAdBIA"
                "AAAAAAAAAAAA/f39/f39/f39/f39/f39/f39/f39/v7+////tbKwdXBthH58"
                "kYyJnpmZrKentra1x8TD1NTT4uLh8PHx////////////////////////////"
                "/////////////////////////////////////v7+/v7+/f39/f39/f39/f39"
                "/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39AP39/f39/f39/f39"
                "/f39/f39/f39/f///3VycEdAPFZNSl5RT1tOTFlMSldKSFRGRFBDQUxAPUk8"
                "OUQ3NUE0Mj4yMEQ6N1JIRV9WVGtkYntzc4mDgpaTkaaiobazssTDwdTT1OXk"
                "5fT09f//////////////////////////////////////////////////////"
                "//////7+/v39/f39/QD9/f39/f39/f39/f39/f39/f39/f3///9kYF5VTkpa"
                "Uk9kWFZjV1VkWFZYS0leUlBhVVNjV1VlWVdlWVdmWVdmWlhlWVdkV1ViVlRg"
                "VFJfUlBcT01ZTEpVSUZTRkNPQkBMPzxIOzlDODZDNjREOTZPQ0FaUU9pYF92"
                "b26Ff36Ujo2jnpyvrau/vL3PzM3b3Nzt7Oz7/Pz////////9/f0A/f39/f39"
                "/f39/f39/f39/f39/f39////aWRiVU5KW1JPZFhWZVlXVUpIVEpHUUhFUENB"
                "TUE/Sj48Rjo4Qjg1QDc0Qzc1RTk3RTk3RTk3RTo4Sz89UERCWExKXFBOXlJQ"
                "YVVTY1ZUZFdWZVlXZVlXZFhWY1dVYVVTYFNRXVBOWk1LV0pIVUhGU0VDT0JA"
                "TD89Sj06Rzo4Oy4r+fr6////AP39/f39/f39/f39/f39/f39/f///7/AwD84"
                "NllST1tST2RYVmVZV1JKR2tfXWpeXGtfXWtfXWtfXWxgXmxgXmxfXWpeXGpe"
                "XGpeXGhcWmRZV11UUVpOTFVJR1FFQ0xAPkg8OUM6OEI6N0Y6OEY6OEI2NEA0"
                "Mj81MkQ4Nkk9O09DQVRIRldLSVxPTV5SUGVZV2JWVGJWVFJFQ+bl5v///wD9"
                "/f39/f39/f39/f39/f3///+6uro8PT1NRkRZUk9bUk9kWFZlWVdTSkdqXlxo"
                "XFppXVtoXFpoXFppXVtiVVNaUlFfVFJnWlhnW1loXFpqXVtmWVdnWlhpXFpp"
                "XVtpXVtrX11sX1xqXVtqXlxqXlxqXlxqXlxoXFpkWlhhVlRdUU9ZTUtUSEZP"
                "Q0FJQD5BNTNlWVdiVlRURkTi4uL///8A/f39/f39/f39/f39////39/fODg4"
                "U1NUTUZEV1BNW1FPZVlXZllYU0pHal5caFxaaV1baV1baV1bYFRSZ2dph4eM"
                "gYKGZWBeZlpXa15cWFBQb3BzcG1vY1hWZlpYaV1bYVRSXlhZY1tbZFdVZlpY"
                "Z1tZaVxaXlJQYFRSZ1pYZ1tZaFxaaV1bZVZXal1cST07ZFhWZFhWVUhG3d3c"
                "////AP39/f39/f39/f39/f///3BwcE9PT1NUVE5HRVhRTltRT2ZZV2ZaWFRM"
                "SGpeXGldW2peXGldW2tfXUg/P4mJjoOChoOChnh3e2haWFFHRXx8gYaFiYSE"
                "iXd2eGVYVmFWUmJhZIeHjIaGi29rbmRYVWldWlZPT3l5fnl6fmVeXmdaWGdb"
                "WWZZWIGSb2pfXEc6OWRYVmNXVVZIRtnZ1////wD9/f39/f39/f3///+QkJA+"
                "Pj43NzdKS0tJQ0FMRUJbUU9mWlhmWlhTSkhrX11qXlxqXlxqXlxsX11ZTUtZ"
                "WVyJiI2Dg4hpZWdpXFpSRkRubnKIiIyFhYl3d3plWVZQRUN1dnqEg4eDgoZ+"
                "f4NjV1RXS0lub3OFhIiDgoZ/gIVjWFVoXFpnWVl+kG5rYl1FOTdkWFZkWFZW"
                "SUfX1NT///8A/f39/f39////+fn5KCgoOzs7LS0tQUJCOzUzLSQhV05LZ1tZ"
                "aFtZVEtIbGBeal5cal5cal5cal9cbWFeXE9OVU5NXVNTaFxZaVxabF9dSEBA"
                "Yl9iZmJlY1pYaFxaZ1pYRkFCgICFfX2CaGRkZllXX1NQVFNViYmOhYWJd3d7"
                "ZVlWaFxaaFxaY09OaVxaRTk3Y1dVY1dVVklH09HQ////AP39/f39/f///9zc"
                "3CMjIyUlJSUlJVdXWEM7OkM8OVlQTmhcWmhcWlVMSmxgXmpeXGtfXWtfXWRV"
                "Vl1QUFxQT1tPTVpQTlxRT2BUUmJYVWhcWWVZVWZaV2dbWGdcWWhdWmdaV1RJ"
                "SFtQT2ldWmldW2xgXVdMSlVQUl9ZW2JZV2lcWmhcWmdYVYu81W1mZ0Q4NWFV"
                "U2RYVldLSNnW1f///wD9/f39/f3////R0dEwMDApKSkqKipWVldHQD5PSUVa"
                "UE1qXlxpXVtWTUpsYF5rX11sYF5lW1eqlp+ij5ejkJeij5aei5OXhYyNe4KF"
                "c3l+bHN4Z21xYmZsXWFpWl9pWlxmWFljVVdgUlJbT05ZTU1ZTUteUk9hVVJk"
                "WFVmW1hnXFlqXlxpXVtlVlJrX1xFOTdhVVNlWVdiVFJsamn///8A/f39/f39"
                "////xsbGKSkpIyMjKioqVFVVSEE/UElGWlBOal5cal5cWE5MbGBea19dbGBe"
                "Y1lWuaevvKqxvqyzwq+2wa+2v620v6y0v620vqyzvauyu6iwt6WstKKpsqCo"
                "sZ6mrZujqpefqJWdppKan4yUlIKJiXZ+fWtxcmFmbFxiVEdIa2BdaV1bbGBe"
                "Rjo4X1NRZVlXZ1pYIyEf////AP39/f39/f///7W1tSMjIzU1NSkpKU9QUEQ9"
                "O0lCP1lQTWtfXWpeXFhOTG1gXmtfXWxgXWNYVsezu6CSmLOjqaGTmq6epMSy"
                "ucKwt8Kwt8Owt7qpsL+ttL+ttL+ttL+ttL+ttMKvt8Cutb6ss72rsryqsb6s"
                "s8WxubimrbWjqpaDi1NFR2xgXmpeXGxgXkU7OV5SUGZaWFtOS7+9vP///wD9"
                "/f39/f3///+pqak1NTVTU1M5OTkiIiM3MS85My9XTkttYF5sYF5YT0xtYV9s"
                "YF5sYF5mW1iunqZ1bXOXiZCfkZeShIrPvcPMusHNusHRvseWio7Itr3MusHL"
                "uL/KuL/Kt7+jlZusnKLItb3Fs7rDsbi8q7JPS03Esbm7qbChj5ZXSUprYF1r"
                "X11tYV9FPDlcUU9nW1lbTkzGwcD///8A/f39/f39////aWlpQUFBTU1NMzMz"
                "IiMjPTY1QDk1WE9MbWFfbGBeWVFObWFfbGBebWFfZVlXyra/wrC3uqmwsaGo"
                "qZuioJKZn5CWnpCVnpCWl4mPmYuRnY+VnI+VnI+UnJCVdW1yhnt/p5meuqmw"
                "xLO6x7S7nI+Vy7jAxLK5rpujWk1PbGBeal5cbmJgRj07WlBOal1bXE9NyMTD"
                "////AP39/f///////w0NDVJSUkxMTDAwMAAAADcwLkQ9OllPTW5iYG1hX1pR"
                "Tm5hX2xgXm5iYGVaWM67w8m3vsy6wdC+xdO/xtO+xtS/x9fBydbAyNvEzdfB"
                "ydfBydbAydbAyNS/x9bByc65wcGutbSiqqiYn6CSl6CSmJmLkZaIjpCAh1xR"
                "UmxgXWtfXW5iYEc+O1lQTWpeXGVYVm5qaf///wD9/f3////6+voiIiJQUFAw"
                "MDAyMjIaGxs5MjBGQDxZT01uYmBuYV9bUk9uYmBtYV9vY2FnXFrBrrjFs7rG"
                "tLvUwMjXwcnRvMTUvse6qK/WwcmajJLItb27qrDGsrrGs7vaxMzRvMTTvsbS"
                "vcXSvcXUvsbSvsbOvMPLucDJt763oqpcT1BsYF5rX11tYV9IPjxYT0xqXlxo"
                "W1lTTk3///8A/f39////9vb2IyMjUlJSKCgoS0tLIyQlODEwR0A9WE5McWVj"
                "cGRiW1JQb2NhbmJgb2Nha19dmIuSybe+opWbmIyRhHyC1r/H18LKpZabrp6k"
                "rZ2krZ2juqivm42SjoSHloiNkIWKyra/073F0bzE1sDI1sDIz73EzrvCx7S7"
                "tJ+nXFBRbWFea19dbmJgSz48WE5Ma19dZ1pYb2tq////AP39/f////r6+ikp"
                "KVBQUDY2NhwcHBARETs0M0Y/PFhPTHJmZHJlY11UUXBkYm9jYW9jYWdbWc+7"
                "xMi2vcGvttbCyc24wNO+xdvEzXx0d7Chp7KiqLGip824wIZ8gLmnr4l/go2C"
                "h825wNO9xdfByoqAhJKHjZmMkpmMkaqco7ijrFxQUWxgXmxgXm9jYUs/PVdN"
                "S21gXmVYVoeCgv///wD///////9SUlI6OjpQUFA+Pj4jIyMUFRU8NTNGQDxY"
                "T0x0aGZyZmReVVJwZGJvY2FwZGJmW1nRvcbLucDQvsXRvcXUvsbTvsbUv8fH"
                "s7rYwsqViY7dx8+rm6Cvn6WSiIyxoKaTiI7WwcnSvcXTvcbLt7+2pqzCsLen"
                "mZ/Esrm4oqtdUlNtYV9sYF5vY2FMQD5WTUtuYmBlWFaZlJP///8A1NTUcXFx"
                "LCwsPj4+UFBQPj4+IyMjFRYWOzQyRT47WVBMdWlndGhmXlVScWVjb2NhcGRi"
                "aF1ayba/yri/yri/077G077G077G1cDIwq+31sLK0r3F0bzEw7C4077G0r7G"
                "2sPM2sTN2MLK2MLL0bzE077G07/GzrzDzLrBx7W8uKSsXlFTbmJfbGBeb2Nh"
                "TUA+WExKbmJgZVlWmJOT////AGRkZAEBAQEBATg4OFFRUT4+PiQkJBcYGDs0"
                "MkU/O1lQTXdqaHVpZ19WU3FlY3BkYnFlY2xgXp2Plo6DiKeYnaGTmdfBydS/"
                "x9nDzKeYnMGwt3VucYuBhaKUmci1vXhwcralrJWIjaubopWJjtjDy9W/x9bB"
                "ydLAx8m3vse1vLmlrV9TVW5jYG1hX29jYU1BP1hMSm9jYWdaWJWQj////wBv"
                "b28AAAAEBAQ6OjpRUVE+Pj4kJCQWGBg7NDJFPjtZT015bWt3a2lfVlRyZmRw"
                "ZGJxZWNoXVrQvMXOvMPSwMfWwcnTvsbUv8fcxs9/d3reyNB5cXSilpyklprd"
                "yNG1pqyilJmRhYlrZWmUiI3iytR7cnWWipCgk5nPvMPHtby4pKtfUlRwZGJu"
                "YmBvY2FOQkBYTEpyZmRqXVuXkZD///8A2tracHBwISEhPDw8UVFRQEBAIiIi"
                "FRYWOzUzRT47WU9Nem5seGxqYVdVcmZkcWVjcWVjaF1b0r7GzbvC0L7F18LL"
                "1L/H1cDI2MPLyLS728bOrp+lv660oZSa4cvTlIeNloqPk4iNn5KXqZuf2MLL"
                "0LvDwK+2wrC3zLrBx7a9uKOrXVJTcWVib2NhcGRiTkJAWExKcmZkal1blY2N"
                "////AP///2xsbEZGRkFBQVJSUjIyMjExMRscHDozMkU+O1lPTXtvbXpta2FY"
                "VXJmZHFlY3JmZGxgXq6gp7KjqMCwt6OUmdjDy9bByd3H0IqAhrCip6WWnLGh"
                "p7KjqsOwuLGiqN3H0NvFzdrEzM66wtS/x9XAyNbAyNG+xcy6wci2vbahqV5T"
                "VHBkYm9jYXFlY1BEQllNS3RoZmxfXZSPjv///wD///9dXV0yMjI2NjZUVFQq"
                "KipLS0skJSU4MTBFPjtYT0x8b216bmxhWFVyZmRyZmRyZmRtYV+vnqeyo6m/"
                "rrWpm6HbxM3Wwcncxs+klZrSvcSLgYXSvcWekZXZxM2jlZujlZnaxc3VwMjV"
                "wMjVv8jMuL/Jtb3QvsXMusHJt763oqteUVNxZWJvY2FzZ2VRRUNZTUt0aGZs"
                "YF2Pi4r///8Abm5uAgICAgICMzMzT09PMTExISEhExQUOTIwRD46WU9OfHBu"
                "em5sYVhVdGhmc2dlcmZkal9c0r/Hz7zE0sDH2MPL1sHJ18LK28bOoZWbhnuA"
                "vqyzdm9zuqmu2cTNqZqgn5OX28bO1cDI1sHJ28XNkIeMz7rC0L/GzLrBybe+"
                "uKSsX1JUcGVib2NhcmZkUkZEWU1LdWlnbmFfkIuK////AGtraxwcHCsrKzk5"
                "OT09PS8vLyAgIBAQETcxL0Q9OllQTXxwbntubGBYVXRnZnNnZXRoZmtgXdK+"
                "x9C+xdXCydfEy9rFzdbBydnDy8y5wOPM1LKjqc67wrCgpuPM1aiZn8+7wt3H"
                "z9bBydXAyNS/x9rDzNS/x8+9xMy6wcm3vrmlrV9TVHJmY3BkYnJmZFJGRFlN"
                "S3ZqaG5hX46JiP///wCwsLBFRUUhISEqKio7OzszMzMlJSUAAAA3Ly4/ODVa"
                "UE58cG57bmxhWFV0aGZ0aGZ1aWdvY2G4pq+snqShlZq0pauyoajaxc3axc61"
                "pKummJ+yoqi2pa2mmJ7Csbehk5nCsLegkpbdx9DVwMjWwcnXwcnTvsbQvsXN"
                "u8LKuL+7pq5eU1RyZmRwZGJyZmRTR0VbT012amhuYV+QiYj///8A////ampq"
                "Pj4+JycnOTk5Ozs7KysrAwQENC0rOTIvWlFOfXFve29tY1dVdWlndWlndmpo"
                "bmNgwK22sqOqyLa+wbG3xLO62cPL3sjQlIqOqJifqJugybe/kIWJ3snSopSZ"
                "mY2Qk4eMxbO62cPL2MPLuqmw1sHJ0L7FzrzDyri/u6auYFRVcmZkcWVjc2dl"
                "U0dFW09NdWlnb2JgjYWF////AP///2NjY0ZGRikpKSYmJiIiIhkZGQMEBDYv"
                "Lj84NVpRTn1xb3tvbWFWVHZqaHZqaHZqaG1iYNO+x9LAx9bDyt7L0+TN1uHL"
                "1OTN1sKwtrSkrIV7f7Wlrcu4v+PN1oV8gKCTl7yrsrenrtrEzNjCyrenrr2s"
                "stLAx868w8q4v72osGBUVXJmZHJmZHNnZVVJR1xQTnVpZ3FkYnZubv///wD/"
                "//9hYWFKSkoyMjIvLy8gICAQEBAAAAA9NTRLREFcU1B8b217bm1fVlN4bGp2"
                "amh3a2lwZGGwoaicj5Wll516cXVuZ2p7cnaGe3+RhoqajJCilJmilJqNg4jE"
                "sbiqm6HNu8KhlJno0Nnkzdbkzdbkzdbfy9PZxs7TwMfPvcS/q7NhVFZzZ2Vy"
                "ZmR0aGZVSkhaUU51aWdzZ2VYUVH///8A////YWFhR0dHTExMPz8/JiYmGxsb"
                "ISIjQTo4SUI/XFJQe25sem5sYVVTeGxqd2tpd2tpbmNg0b7GzrzD3cnRfXN2"
                "TUpKUk1OUU1NTElJcWlugXh8jICFb2ZqcWptbmZpZ2BjYVtfWFJVUExNWlVX"
                "Zl5gbWVofXN2pJacnZCVk4SMZFdZc2dlcmZkdGhmV0tJW1JPdmlndmlnNy8v"
                "////AP///2BgYEdHR0lJSSoqKhsbGxkZGUdISEI7OkQ+OltST3pta3lta19T"
                "UXlta3draXhsam9kYdK+x8+8xN3K0n10d0tISVBNTVBMTUxISIB1eWhgZHhw"
                "c3tzeIV6f4l+g42Ahp2QlXFoa1BLTFJOTlJNTk5KS2JcXtzJ0c67w7unr15S"
                "VHRoZnNnZXVoZldMSlxSUHRoZmxfXamko////wD///9gYGBHR0dJSUlLS0tX"
                "V1c7Ozs7Ozw2Ly0tIyFaUU93a2l3a2leUlB6bmx3a2l4bGp2amh6bW2EdnmJ"
                "fX+bi46jkZagkJafj5SbjpOUh46Qho2RhYmNgIeGfICBdnp4cHRwaWxsZWln"
                "YmNgWVtWUlNMSElfWlzdyNDMusG6pq9gU1d0aWZzZ2V2amhYTEpcU1BzZ2Vp"
                "XFqrp6b///8A////YGBgRkZGPT09S0tLU1NTUVFRRkdHPjc1OjMwW1JPdWhm"
                "dGhmW1JPem5seGxqc2Zkb2Jgraimf3RyeXFufXRxdmtpdGhldWpndGhldGhl"
                "dGhlc2dldmlneWxsfHBvfnFwg3Z2iHt9kYGDloaJnIuQoZGWnY6SoJGVpJSa"
                "l4eOWk9Qdmpoc2dldmpoWE5MXVNRcmZkaFxZtK+u////AP///15eXj4+PklJ"
                "SUhISEhISEhISEZHR0hBQExFQlxTUHNnZXJlZFlQTXpubHRpZ6qko5aQjrOv"
                "r7ezsp6Yl5SNi5CIh5CJhoB4dXZpaHhsanhsandraXdraXdraXVpZ42Bf4V4"
                "doBzcXtubHZraHNnZG5hX21hXmldWmdbWGpeW3BkYXFlY3JmZHZpZ1pOTF1U"
                "UXBkYm1gXmBaWe/w8AD///9SUlJERERJSUlJSUlJSUlKSkpHSEg9NjRLREFb"
                "UlBwY2FvY2FYT0x7bm1zaWbZ2NeRiYjGxMOsp6euqqnBvb3Gw8O9vLuqpKNz"
                "ZmR4bGp4bGp4bGp4bGp2amh6bmyxpaPJwsLMx8XSzs3JwcHLxcPT0M+toqG/"
                "trbGwL+5sbC3r62bj42EeHZ0aGZcUE5eUlBtYV9uYmA4MDDa29sA////R0dH"
                "OTk5SEhISUlJTExMREREFxgYPzg2S0RBW1JQbWFfbWFfWE5Ld2tpe25sdGdl"
                "eWxqdmlndmpndWhmfHFugHZzc2Zjdmpoe29tem5sem5seW1reW1reGxqdmpo"
                "joKAjoKAkYSClIeFmo6Mm46MopeUsammsaelt66surCuwrq5rKCelIiGc2dl"
                "XVFPX1NRa19dY1ZUqqal////AP////f399TU1Do6Ok9PTzU1NREREUlKSkY/"
                "PUpDQFtSUGteXWldW2xgXlRIRlJGRFJGQ1JGRFRIRlVJR1ZKSFZKSFdKSFpO"
                "TFtPTV9TUWRYVmpeXG9jYXNnZXZqaHhsanhsanhsandraXdraXZqaHVpZ3Ro"
                "ZnNmZXNmZHNnZXVoZndqaHxwbnhsandraV5SUF9TUWldW19SUK6qqf///wD+"
                "/v7///+Xl5dGRkYhISEeHh5OTk5GR0dFPjxLREFYTkxjV1ViVlRiVlRkWFZk"
                "WFZkWFZlWVdmWlhmWlhnW1loXFpoXFpoXFpmWlhkWFZgVFJbT01XS0lWSkhS"
                "SEVRRUNRRUNSRkRTR0VTR0VVSUdWSkhXS0lYTEpaTkxbT01fU1FkWFZoXVtu"
                "Y2BzZ2VZTUtiVlRmWlhcT02vqqr///8A/v7+////lpaWAgICMDAwTU1NR0dH"
                "QkNDQzs6Qzs4b2Jhem5sd2tpdWlndGdlcWVjbmJgal5cZlpYY1dVYFRSXlJQ"
                "XVFPXVFPXFBOXVFPXVFPXlJQX1NRX1NRX1NRYFRSYFRSYVVTYlZUY1dVZFhW"
                "ZVlXZlpYZlpYZVlXZVlXYVVTXlJQWE1LU0hGU0dFU0hGZlpYY1dVWk1LsKuq"
                "////AP7+/v///4mJiSwsLEtLS0ZGRj4+PlFSUk9GRXJnZYZ5d4R5doJ1c4V5"
                "d4J1c4R3dX9zcYF0coN3dYR4doV5d4R4doN3dYF2dH90cX5ycHtvbXhsanVp"
                "Z3NnZXFlY29jYW5iYGxgXmldW2RYVmBUUl1RT1xQTltPTVpOTFpOTFpOTFlN"
                "S1tPTVxQTlxQTl1RT1xQTlxQTlNGRLCrq////wD+/v7////Hx8c4ODhDQ0M+"
                "Pj5hYWF3d3dbW1tZVFRzbm5LRkZ+eHdNSEV3cW9YUVCZkI6OhIOEeniBdnV8"
                "cG15bGp4bGl3amd2aWd2amd4bWqBdHKCdXOEeHaFeHaFeXd5bGpmWVdqXVtu"
                "YmB0aGZyZmR0aGZ4bGp4bGp3a2l5bWt5bWt4bGp2amhwZGJtYV9rX11oXFpY"
                "S0m5tLP///8A/v7+/v7+////KSkpQ0NDbGxsY2NjQEBAWVlZV1hYSEhIZ2ho"
                "NDU1Y2NkYWJizc/P7O7u7e/v////zs/Pra6uvL69ubq6y8vL1dTU3drawb6/"
                "cGxrdXFvWVVTUktKZFpaVExLU0pJWE9NXlNRY1hVY1ZUY1ZUZ1pXXE9NWUxK"
                "YFNRWEtIWEtJXE9Nem1reGxqeGxqd2podmlo////////AP7+/v7+/v///2Fh"
                "YXh4eGlpaTw8PFxcXDU1NU1NTURERD4+Pl9fX5WVlfr6+tXV1bq8vNXW1XFx"
                "cSAgICoqKioqKlBQUGdoaEREREZHR1dYWEFCQmpqazEyMm9wcBAREQAAAA0O"
                "DhMUFBETExETExIUFBcXFx0cHSUkJSspKjEuLTYzMjo3NjozMomFhLKrq6Ga"
                "mZaOjfr7+/////7+/gD+/v7+/v7+/v7////////////////////////29vbt"
                "7e3g4ODp6en///////////////////9sbGwwMDBGRkZubm5eXl47OztiYmJG"
                "RkZZWVlUVFRJSUleXl5EREQkJCQCAgIUFBQaGhoaGhoZGRkaGhoZGRkYGBgX"
                "GBgWFxcWFhYVFhYVFRUEBQWmp6f////////////////+/v7+/v4A/v7+/v7+"
                "/v7+/v7+/v7+/v7+/v7+/v7+/////////////////////v7+/v7+/v7+/v7+"
                "////eHh4QUFBYmJiXFxcPDw8ZGRkMjIyYGBgNjY2WVlZQUFBT09PVVVVCAgI"
                "AwMDGRkZISEhICAgICAgHx8fHx8fIiIiHx8fHx8fISEhISEhHx8fDQ0Nl5eX"
                "/////v7+/v7+/v7+/v7+/v7+AP7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+"
                "/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v////X19enp6d/f39fX18nJ"
                "ycLCwrS0tKysrJ+fn5aWloqKin5+fnV1dRkZGQMDAxMTExEREQAAABsbGxYW"
                "FgICAhgYGBkZGRERERERERsbGwkJCf////////7+/v7+/v7+/v7+/v7+/gD9"
                "/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39/f39"
                "/f39/f39/f3+/v7/////////////////////////////////////////////"
                "///////U1NScnJyJiYmysrJqampXV1d7e3s2NjYvLy8sLCwmJiYAAAAAAABa"
                "Wlr////+/v79/f39/f39/f39/f39/f0A/v7+/v7+/v7+/v7+/v7+/v7+/v7+"
                "/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+"
                "/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+/v7+////////////////////"
                "/////////////////////////////////////v7+/v7+/v7+/v7+/v7+/v7+"
                "/v7+AP//////////////////////////////////////////////////////"
                "////////////////////////////////////////////////////////////"
                "////////////////////////////////////////////////////////////"
                "/////////////////////////////////////wA=";

[Device Classification]
        Class1 = EtherNetIP;

[Params]
        Param1 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 3000
                "Current A",            $ name
                "2 bytes",              $ units
                "Current A",            $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param2 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 3002
                "Current B",            $ name
                "2 bytes",              $ units
                "Current B",            $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param3 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 3004
                "Current C",            $ name
                "2 bytes",              $ units
                "Unit Identifier String",    $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param4 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 3006
                "Current N",            $ name
                "2 bytes",              $ units
                "Current N",            $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param5 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 3008
                "Current G",            $ name
                "2 bytes",              $ units
                "Unit Identifier String",    $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param6 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 30010
                "Current Avg",          $ name
                "2 bytes",              $ units
                "",                     $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param7 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register 3012
                "Current Unbalance A",  $ name
                "2 bytes",              $ units
                "Current Unbalance A",  $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param8 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register address 3014
                "Current Unbalance B",  $ name
                "2 bytes",              $ units
                "Current Unbalance B",  $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param9 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register 3016
                "Current Unbalance C",  $ name
                "2 bytes",              $ units
                "Current Unbalance C",  $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param10 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register 3018
                "Current Unbalance Worst",    $ name
                "2 bytes",              $ units
                "Current Unbalance Worst",    $ help string
                $ Should be a 14 byte string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

        Param11 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register 3020
                "Voltage A-B",          $ name
                "",                     $ units
                "",                     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param12 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register 3022
                "Voltage B-C",          $ name
                "",                     $ units
                "Voltage B-C",          $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param13 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                $ Register 3024
                "Voltage C-A",          $ name
                "",                     $ units
                "Voltage C-A",          $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param14 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage L-L Avg",      $ name
                "",                     $ units
                "Voltage L-L Avg",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param15 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage A-N",          $ name
                "",                     $ units
                "",                     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param16 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage B-N",          $ name
                "",                     $ units
                "",                     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param17 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage C-N",          $ name
                "",                     $ units
                "New Help String",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param18 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "--",                   $ name
                "",                     $ units
                "New Help String",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param19 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage L-N Avg",      $ name
                "",                     $ units
                "New Help String",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param20 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalanced A-B",    $ name
                "",                     $ units
                "",                     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param21 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalanced B-C",    $ name
                "",                     $ units
                "Voltage Unbalanced B-C",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param22 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalanced C-A",    $ name
                "",                     $ units
                "Voltage Unbalanced C-A",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param23 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalance L-L Worst",    $ name
                "",                     $ units
                "Voltage Unbalance L-L Worst",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param24 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalance A-N",$ name
                "",                     $ units
                "Voltage Unbalance A-N",$ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param25 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalance B-N",$ name
                "",                     $ units
                "Voltage Unbalance B-N",$ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param26 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalance C-N",$ name
                "",                     $ units
                "Voltage Unbalance C-N",$ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param27 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Voltage Unbalance L-N Worst",    $ name
                "",                     $ units
                "New Help String",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param28 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Power A",       $ name
                "",                     $ units
                "Active Power A",       $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param29 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Power B",       $ name
                "",                     $ units
                "Active Power B",       $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param30 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Power C",       $ name
                "",                     $ units
                "Active Power C",       $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param31 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Power total",   $ name
                "",                     $ units
                "Active Power total",   $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param32 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Power A",     $ name
                "",                     $ units
                "Reactive Power A",     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param33 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Power B",     $ name
                "",                     $ units
                "Reactive Power B",     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param34 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Power C",     $ name
                "",                     $ units
                "Reactive Power C",     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param35 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Power Total", $ name
                "",                     $ units
                "",                     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param36 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apperent Power A",     $ name
                "",                     $ units
                "Apperent Power A",     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param37 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apperent Power B",     $ name
                "",                     $ units
                "Apperent Power B",     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param38 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apperent Power C",     $ name
                "",                     $ units
                "Apperent Power C",     $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param39 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apperent Power Total", $ name
                "",                     $ units
                "Apperent Power Total", $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param40 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Power Factor A",       $ name
                "",                     $ units
                "Power Factor A",       $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param41 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Power Factor B",       $ name
                "",                     $ units
                "Power Factor B",       $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param42 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Power Factor C",       $ name
                "",                     $ units
                "New Help String",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param43 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Power Factor Total",   $ name
                "",                     $ units
                "Power Factor Total",   $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param44 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Displacement Power Factor A",    $ name
                "",                     $ units
                "Displacement Power Factor A",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param45 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Displacement Power Factor B",    $ name
                "",                     $ units
                "Displacement Power Factor B",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param46 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Displacement Power Factor C",    $ name
                "",                     $ units
                "Displacement Power Factor C",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param47 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Displacement Power Factor Total",    $ name
                "",                     $ units
                "Displacement Power Factor Total",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param48 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Frequency",            $ name
                "",                     $ units
                "Frequency",            $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param49 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Energy Delivered (Into Load)",    $ name
                "",                     $ units
                "Active Energy Delivered (Into Load)",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param50 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Energy Received (Out of Load)",    $ name
                "",                     $ units
                "Active Energy Received (Out of Load)",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param51 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Energy Delivered + Received",    $ name
                "",                     $ units
                "Active Energy Delivered + Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param52 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Active Energy Delivered- Received",    $ name
                "",                     $ units
                "Active Energy Delivered- Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param53 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Energy Delivered",    $ name
                "",                     $ units
                "Reactive Energy Delivered",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param54 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Energy Received",    $ name
                "",                     $ units
                "Reactive Energy Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param55 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Energy Delivered + Received",    $ name
                "",                     $ units
                "Reactive Energy Delivered + Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param56 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Reactive Energy Delivered - Received",    $ name
                "",                     $ units
                "Reactive Energy Delivered - Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param57 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apparent Energy Delivered",    $ name
                "",                     $ units
                "Apparent Energy Delivered",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param58 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apparent Energy Received",    $ name
                "",                     $ units
                "Apparent Energy Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param59 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apparent Energy Delivered + Received",    $ name
                "",                     $ units
                "Apparent Energy Delivered + Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param60 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Apparent Energy Delivered - Received",    $ name
                "",                     $ units
                "Apparent Energy Delivered - Received",    $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param61 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI",                  $ name
                "",                     $ units
                "New Help String",      $ help string
                100000,10000000,1000000,$ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param62 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "Connection Instance O->T Output ",    $ name
                "",                     $ units
                "New Help String",      $ help string
                150,150,150,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param63 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xC6,                   $ Data Type
                1,                      $ Data Size in bytes
                "Connection Instance T->O Input",    $ name
                "",                     $ units
                "",                     $ help string
                100,100,100,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param64 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Size T->O Input",      $ name
                "",                     $ units
                "",                     $ help string
                240,240,240,            $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param65 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "Size O->T Output",     $ name
                "",                     $ units
                "",                     $ help string
                4,4,4,                  $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param67 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xCA,                   $ Data Type
                4,                      $ Data Size in bytes
                "Dummy Parameter for Output assembly",    $ name
                "",                     $ units
                "New Help String",      $ help string
                ,,0,                    $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

[Assembly]
        Object_Name = "Assembly Object";
        Object_Class_Code = 0x04;
        Assem1 =
                "Input Assembly",
                ,
                240,
                0x0000,
                ,,
                32,Param1,
                32,Param2,
                32,Param3,
                32,Param4,
                32,Param5,
                32,Param6,
                32,Param7,
                32,Param8,
                32,Param9,
                32,Param10,
                32,Param11,
                32,Param12,
                32,Param13,
                32,Param14,
                32,Param15,
                32,Param16,
                32,Param17,
                32,Param18,
                32,Param19,
                32,Param20,
                32,Param21,
                32,Param22,
                32,Param23,
                32,Param24,
                32,Param25,
                32,Param26,
                32,Param27,
                32,Param28,
                32,Param29,
                32,Param30,
                32,Param31,
                32,Param32,
                32,Param33,
                32,Param34,
                32,Param35,
                32,Param36,
                32,Param37,
                32,Param38,
                32,Param39,
                32,Param40,
                32,Param41,
                32,Param42,
                32,Param43,
                32,Param44,
                32,Param45,
                32,Param46,
                32,Param47,
                32,Param48,
                32,Param49,
                32,Param50,
                32,Param51,
                32,Param52,
                32,Param53,
                32,Param54,
                32,Param55,
                32,Param56,
                32,Param57,
                32,Param58,
                32,Param59,
                32,Param60;
        Assem2 =
                "Output Assembly",
                ,
                4,
                0x0000,
                ,,
                32,Param67;

[Connection Manager]
        Revision = 1;
        Object_Name = "Connection Manager Object";
        Object_Class_Code = 0x06;
        MaxInst = 1;
        Connection1 =
                0x04010002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = transport type: listen-only
                                        $ 25      = transport type: input-only
                                        $ 26      = transport type: exclusive-owner
                                        $ 27      = transport type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Client = 0 / Server = 1
                0x77640405,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param61,Param65,Assem2, $ O->T RPI, size, format
                Param61,Param64,Assem1, $ T->O RPI, size, format
                ,,                      $ config #1 size, format
                ,,                      $ config #2 size, format
                "Class 1 Connection",   $ Connection Name
                "",                     $ help string
                "20 04 24 01 2C 96 2C 64";    $ Path

[Port]
        Revision = 1;
        Object_Name = "Port Object";
        Object_Class_Code = 0xF4;
        MaxInst = 1;
        Port1 =
                TCP,
                "EtherNet/IP Port",
                "20 F5 24 01",
                02,
                03,
                ;

[Capacity]
        TSpec1 =
                TxRx,
                240,
                $ Calculated with RPI 100.
                1;

[TCP/IP Interface Class]
        Revision = 3;
        Object_Name = "TCP/IP Interface Object";
        Object_Class_Code = 0xF5;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;

[Ethernet Link Class]
        Revision = 3;
        Object_Name = "Ethernet Link Object";
        Object_Class_Code = 0xF6;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        InterfaceLabel1 = "Port1";
        InterfaceLabel2 = "Port2";

