,TS Frame##Other##,Ampere Ratings##Other##,Basic Transfer Type##Other##,Poles##Other##,Neutral Type##Other##,UL Enclosure Type Rating##Other##,Mounting Type##Other##,H##Length##Inches,W##Length##Inches,D##Length##Inches,Ventilation Location##Other##,Conductor Entry##Other##,Power Terminal Conductor Range Phase and N (Al/Cu)##Other##,Power Terminal Locations##Other##,Ground Terminal Conductor Range (Al/Cu)##Other##,Ground Bus 20 Percent Rated##Other##,Model Number##Other##
2600A-Open Transition Transfer & Bypass-Isolation Switch-2P,G,2600,TB,2,"None,Solid,Switched,Overlapping",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TB-2600-2P
2600A-Open Transition Transfer & Bypass-Isolation Switch-3P,G,2600,TB,3,"None,Solid,Switched,Overlapping",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TB-2600-3P
3000A-Open Transition Transfer & Bypass-Isolation Switch-2P,G,3000,TB,2,"None,Solid,Switched,Overlapping",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TB-3000-2P
3000A-Open Transition Transfer & Bypass-Isolation Switch-3P,G,3000,TB,3,"None,Solid,Switched,Overlapping",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,TB-3000-3P
2600A-Delayed Transition Transfer & Bypass-Isolation Switch-2P,G,2600,DTB,2,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTB-2600-2P
2600A-Delayed Transition Transfer & Bypass-Isolation Switch-3P,G,2600,DTB,3,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTB-2600-3P
3000A-Delayed Transition Transfer & Bypass-Isolation Switch-2P,G,3000,DTB,2,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTB-3000-2P
3000A-Delayed Transition Transfer & Bypass-Isolation Switch-3P,G,3000,DTB,3,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,DTB-3000-3P
2600A-Closed Transition Transfer & Bypass-Isolation Switch-2P,G,2600,CTB,2,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTB-2600-2P
2600A-Closed Transition Transfer & Bypass-Isolation Switch-3P,G,2600,CTB,3,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTB-2600-3P
3000A-Closed Transition Transfer & Bypass-Isolation Switch-2P,G,3000,CTB,2,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTB-3000-2P
3000A-Closed Transition Transfer & Bypass-Isolation Switch-3P,G,3000,CTB,3,"None,Solid,Switched",1,Free Standing,91,38,72,Front/Rear,Top & Bottom,(10) 1/0 - 750 MCM ,Rear,(36) 1/0 - 750 MCM,1,CTB-3000-3P
